Inventory Report for the XenServer Pool: XenServer DC1

Table of Contents

[XenServer DC1 Pool 4](#_Toc140039087)

[General 4](#_Toc140039088)

[Custom Fields 4](#_Toc140039089)

[Email Options 4](#_Toc140039090)

[Power On 4](#_Toc140039091)

[Live Patching 4](#_Toc140039092)

[Network Options 4](#_Toc140039093)

[Clustering 4](#_Toc140039094)

[Updates 4](#_Toc140039095)

[Management Interfaces 6](#_Toc140039096)

[Hosts 7](#_Toc140039097)

[Host: xs01 7](#_Toc140039098)

[Custom Fields 7](#_Toc140039099)

[Power On 7](#_Toc140039100)

[License Details 7](#_Toc140039101)

[Version Details 7](#_Toc140039102)

[Management Interface 7](#_Toc140039103)

[Memory 7](#_Toc140039104)

[CPUs 8](#_Toc140039105)

[Networking 8](#_Toc140039106)

[NICs 8](#_Toc140039107)

[GPU 8](#_Toc140039108)

[Host: xs02 8](#_Toc140039109)

[Custom Fields 9](#_Toc140039110)

[Power On 9](#_Toc140039111)

[License Details 9](#_Toc140039112)

[Version Details 9](#_Toc140039113)

[Management Interface 9](#_Toc140039114)

[Memory 9](#_Toc140039115)

[CPUs 9](#_Toc140039116)

[Networking 9](#_Toc140039117)

[NICs 10](#_Toc140039118)

[GPU 10](#_Toc140039119)

[Virtual Machines 11](#_Toc140039120)

[VM: VM1 11](#_Toc140039121)

[Network 11](#_Toc140039122)

[GPU 11](#_Toc140039123)

[Custom Fields 11](#_Toc140039124)

[VM: VM2 11](#_Toc140039125)

[Network 11](#_Toc140039126)

[GPU 11](#_Toc140039127)

[Custom Fields 11](#_Toc140039128)

[VM: VM3 12](#_Toc140039129)

[Network 12](#_Toc140039130)

[GPU 12](#_Toc140039131)

[Custom Fields 12](#_Toc140039132)

# XenServer DC1 Pool

## General

|  |  |
| --- | --- |
| **Pool name** | XenServer DC1 |
| **Description** | DC1 XenServer Pool |
| **Tags** | <None> |
| **Folder** | None |
| **Pool License** | Express |
| **Number of Sockets** | 4 |
| **XenServer Version** | 8.2 CU1 |
| **UUID** | cbc7525a-8e4e-ee92-4672-5a426de9a4f9 |

## Custom Fields

There are no Custom Fields for Pool XenServer DC1

## Email Options

Send email alert notifications is disabled

## Power On

|  |  |
| --- | --- |
| **Server** | xs01 |
| **Power On mode** | Disabled |
|  |  |
| **Server** | xs02 |
| **Power On mode** | Disabled |
|  |  |

## Live Patching

Live patching is Enabled

## Network Options

IGMP snooping is Disabled

## Clustering

Clustering is Disabled

## Updates

| **Fully applied** |
| --- |
| CH82ECU1 (version 1.0) |
| XS82ECU1001 (version 1.0) |
| XS82ECU1002 (version 1.0) |
| XS82ECU1003 (version 1.0) |
| XS82ECU1004 (version 1.0) |
| XS82ECU1005 (version 1.0) |
| XS82ECU1006 (version 1.0) |
| XS82ECU1007 (version 1.0) |
| XS82ECU1008 (version 1.0) |
| XS82ECU1009 (version 1.0) |
| XS82ECU1010 (version 1.0) |
| XS82ECU1011 (version 1.0) |
| XS82ECU1012 (version 1.0) |
| XS82ECU1013 (version 1.0) |
| XS82ECU1014 (version 1.0) |
| XS82ECU1015 (version 1.0) |
| XS82ECU1016 (version 1.0) |
| XS82ECU1017 (version 1.0) |
| XS82ECU1018 (version 1.0) |
| XS82ECU1019 (version 1.0) |
| XS82ECU1020 (version 1.0) |
| XS82ECU1021 (version 1.0) |
| XS82ECU1022 (version 1.0) |
| XS82ECU1023 (version 1.0) |
| XS82ECU1024 (version 1.0) |
| XS82ECU1026 (version 1.0) |
| XS82ECU1027 (version 1.0) |
| XS82ECU1028 (version 1.0) |
| XS82ECU1030 (version 1.0) |
| XS82ECU1031 (version 1.0) |
| XS82ECU1032 (version 1.0) |
| XS82ECU1034 (version 1.0) |

## Management Interfaces

|  |  |
| --- | --- |
| DNS hostname on xs01: | xs01 |
| Management interface on xs01: | 192.168.182.11 |
| DNS hostname on xs02: | xs02 |
| Management interface on xs02: | 192.168.182.12 |

# Hosts

## Host: xs01

|  |  |
| --- | --- |
| **Name** | xs01 |
| **Description** | Default install |
| **Tags** | <None> |
| **Pool master** | Yes |
| **Folder** | None |
| **Enabled** | True |
| **iSCSI IQN** | iqn.2023-07.com.example:f07f2a63 |
| **Log destination** | Local |
| **Server uptime** | 5 days, 8 hours, 2 minutes |
| **Toolstack uptime** | 5 days, 8 hours, 2 minutes |
| **Domain** |  |
| **UUID** | 991e2a04-aae7-4dbc-8cb0-b4be211a9f94 |

### Custom Fields

### Power On

|  |  |
| --- | --- |
| **Server** | xs01 |
| **Power On mode** | Disabled |

### License Details

|  |  |
| --- | --- |
| **Status** | Unlicensed |
| **License** | Citrix Hypervisor Express Edition |
| **Number of Sockets** | 2 |
| **License Server Address** | localhost |
| **License Server Port** | 27000 |

### Version Details

|  |  |
| --- | --- |
| **Build date** | 2023-03-09 |
| **Version** | 8.2 CU1 |
| **DBV** | 2020.0617 |

### Management Interface

|  |  |
| --- | --- |
| **DNS hostname** | xs01 |
| **Management interface** | 192.168.182.11 |

### Memory

|  |  |
| --- | --- |
| **Server** | 2.2 GB RAM available (8.0 GB) |
| **VMs** | 2 |
|  | VM1: using 2.0 GB |
|  | VM2: using 2.0 GB |
| **Citrix Hypervisor** | 1.8 GB |
| **Control domain memory** | 1.4 GB |
| **Available memory** | 2.2 GB |
| **Total max memory** | 5.8 GB (72% of total memory) |

### CPUs

|  |  |
| --- | --- |
| **CPU** | 0 - 3 |
| **Vendor** | GenuineIntel |
| **Model** | 13th Gen Intel(R) Core(TM) i9-13900H |
| **Speed** | 2996 MHz |

### Networking

|  |  |
| --- | --- |
| **Number of networks** | 1 |
| **Name** | Netw0 |
| **Description** |  |
| **NIC** | NIC 0 |
| **VLAN** | - |
| **Auto** | Yes |
| **Link Status** | Connected |
| **MAC** | 00:0c:29:82:08:db |
| **MTU** | 1500 |

### NICs

|  |  |
| --- | --- |
| **Number of NICs** | 1 |
| **NIC** | NIC 0 |
| **MAC** | 00:0c:29:82:08:db |
| **Link Status** | Connected |
| **Speed** | 1000 Mbit/s |
| **Duplex** | Full |
| **Vendor** | Intel Corporation |
| **Device** | 82545EM Gigabit Ethernet Controller (Copper) |
| **PCI Bus Path** | 0000:02:01.0 |
| **FCoE Capable** |  |
| **SR-IOV Capable** |  |

### GPU

|  |  |
| --- | --- |
| **Number of GPU's Installed** | 1 |
|  |  |
| **Name** | Group of VMware SVGA II Adapter GPUs |
| **vGPU allocation** | Maximum density (depth\_first) |
| **Primary host display adapter** | True |
| **vGPU Pofiles** | none |

## Host: xs02

|  |  |
| --- | --- |
| **Name** | xs02 |
| **Description** | Default install |
| **Tags** | <None> |
| **Pool master** | No |
| **Folder** | None |
| **Enabled** | True |
| **iSCSI IQN** | iqn.2023-07.com.example:d39ff04f |
| **Log destination** | Local |
| **Server uptime** | 4 days, 19 hours, 19 minutes |
| **Toolstack uptime** | 4 days, 19 hours, 19 minutes |
| **Domain** |  |
| **UUID** | 6bb1e5a2-562e-4808-a34d-63e73f8f24df |

### Custom Fields

### Power On

|  |  |
| --- | --- |
| **Server** | xs02 |
| **Power On mode** | Disabled |

### License Details

|  |  |
| --- | --- |
| **Status** | Unlicensed |
| **License** | Citrix Hypervisor Express Edition |
| **Number of Sockets** | 2 |
| **License Server Address** | localhost |
| **License Server Port** | 27000 |

### Version Details

|  |  |
| --- | --- |
| **Build date** | 2023-03-09 |
| **Version** | 8.2 CU1 |
| **DBV** | 2020.0617 |

### Management Interface

|  |  |
| --- | --- |
| **DNS hostname** | xs02 |
| **Management interface** | 192.168.182.12 |

### Memory

|  |  |
| --- | --- |
| **Server** | 6.3 GB RAM available (8.0 GB) |
| **VMs** | 0 |
| **Citrix Hypervisor** | 1.8 GB |
| **Control domain memory** | 1.4 GB |
| **Available memory** | 6.2 GB |
| **Total max memory** | 1.8 GB (22% of total memory) |

### CPUs

|  |  |
| --- | --- |
| **CPU** | 0 - 3 |
| **Vendor** | GenuineIntel |
| **Model** | 13th Gen Intel(R) Core(TM) i9-13900H |
| **Speed** | 2995 MHz |

### Networking

|  |  |
| --- | --- |
| **Number of networks** | 1 |
| **Name** | Netw0 |
| **Description** |  |
| **NIC** | NIC 0 |
| **VLAN** | - |
| **Auto** | Yes |
| **Link Status** | Connected |
| **MAC** | 00:50:56:22:24:88 |
| **MTU** | 1500 |

### NICs

|  |  |
| --- | --- |
| **Number of NICs** | 1 |
| **NIC** | NIC 0 |
| **MAC** | 00:50:56:22:24:88 |
| **Link Status** | Connected |
| **Speed** | 1000 Mbit/s |
| **Duplex** | Full |
| **Vendor** | Intel Corporation |
| **Device** | 82545EM Gigabit Ethernet Controller (Copper) |
| **PCI Bus Path** | 0000:02:01.0 |
| **FCoE Capable** |  |
| **SR-IOV Capable** |  |

### GPU

|  |  |
| --- | --- |
| **Number of GPU's Installed** | 1 |
|  |  |
| **Name** | Group of VMware SVGA II Adapter GPUs |
| **vGPU allocation** | Maximum density (depth\_first) |
| **Primary host display adapter** | True |
| **vGPU Pofiles** | none |

# Virtual Machines

## VM: VM1

|  |  |
| --- | --- |
| **VM name** | VM1 |
| **Xen host name** | xs01 |
| **VM Operating System** | N/A |
| **Number of vCPUs** | 2 (1 socket with 2 cores) |
| **Memory** | 2 GB |
| **Boot order** | [1] Disk, [2] DVD-drive |
| **Boot mode** | UEFI |
| **Secure boot** | False |

### Network

|  |  |
| --- | --- |
| **Number of NICs** | 1 |
| **Device** | 0 |
| **MAC address** | 42:3b:09:ac:92:30 |
| **MAC autogenerated** | True |
| **MTU size** | 1500 |
| **Network name** | Netw0 |

### GPU

There are no GPU's configured for VM VM1

### Custom Fields

There are no Custom Fields for VM VM1

## VM: VM2

|  |  |
| --- | --- |
| **VM name** | VM2 |
| **Xen host name** | xs01 |
| **VM Operating System** | N/A |
| **Number of vCPUs** | 2 (1 socket with 2 cores) |
| **Memory** | 2 GB |
| **Boot order** | [1] Disk, [2] DVD-drive |
| **Boot mode** | UEFI |
| **Secure boot** | False |

### Network

|  |  |
| --- | --- |
| **Number of NICs** | 1 |
| **Device** | 0 |
| **MAC address** | ca:8d:6c:38:f8:f4 |
| **MAC autogenerated** | True |
| **MTU size** | 1500 |
| **Network name** | Netw0 |

### GPU

There are no GPU's configured for VM VM2

### Custom Fields

There are no Custom Fields for VM VM2

## VM: VM3

|  |  |
| --- | --- |
| **VM name** | VM3 |
| **Xen host name** | N/A |
| **VM Operating System** | N/A |
| **Number of vCPUs** | 2 (1 socket with 2 cores) |
| **Memory** | 4 GB |
| **Boot order** | [1] Disk, [2] DVD-drive |
| **Boot mode** | UEFI |
| **Secure boot** | False |

### Network

|  |  |
| --- | --- |
| **Number of NICs** | 1 |
| **Device** | 0 |
| **MAC address** | f2:ac:9a:58:64:b7 |
| **MAC autogenerated** | True |
| **MTU size** | 0 |
| **Network name** | Netw0 |

### GPU

There are no GPU's configured for VM VM3

### Custom Fields

There are no Custom Fields for VM VM3